;
; OEMSETUP.INF for the yuknd.dos v7.05 NDIS2 driver supporting the
; Marvell Yukon Ethernet Controller.
;
; (C)Copyright 2003-2004 Marvell(R).
; All rights reserved.
;

[disks]

[netcard]
MRVL$yuknd="Marvell Yukon Ethernet Controller",0,ndis,ethernet,real,MRVL$yuknd,MRVL$yuknd_nif

[MRVL$yuknd]
devdir=?:yuknd.dos
device=yuknd.dos,@devdir\yuknd.dos

[MRVL$yuknd_nif]
DriverName="yuknd$"
param=FIX,"FIX (see readme)",static,"2",2,0x30
param=CONTYPE,"Connection Type",text,"AUTO,_100FD,_100HD,_10FD,_10HD","AUTO",0x32
param=CHECKLINK,"Use First Link Found",int,"0,1,1",0,0x32
param=BUSNUM,"Adapter's PCI Bus Number",int,"0,255,1",0,0x32
param=DEVNUM,"Adapter's PCI Device Number",int,"0,31,1",0,0x32
param=MAXRECEIVES,"Number of Receive Buffers",int,"1,4,1",2,0x32
param=MAXTRANSMITS,"Number of Transmit Buffers",int,"1,4,1",2,0x32
