;DrIvEr DeScRiPtIoN
;CoPyRiGhT=(C)Copyright Marvell. All rights reserved

VER:	1.17
SYN:	1.00

DR YUKONNW
{
	DES:		$YUKONNW_DES
	HELP:		$YUKONNW_HLP
	PAR:		2.00
	PROD:		'PCI.11AB.4320.*.*.*',
				'PCI.11AB.4360.*.*.*',
				'PCI.11AB.4361.*.*.*',
				'PCI.11AB.4362.*.*.*',
				'PCI.11AB.4350.*.*.*'

	;@#	SPROD:	'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Fast Ethernet 10/100Base-T Controller'
	;@#	CLIENT:	YUKONNW.LAN
	;@#	ALIAS:	YUKONNW.LAN
	FILE:		YUKONNW.LAN
;	OF:			NBI.NLM, MSM.NLM, ETHERTSM.NLM
	TIME:		15

	PR SLOT REQ
	{
		VAL:	1-65535
	}

	PR NODE OPT
	{
		DES:	$NODE_DES
		HELP:	$NODE_HLP
		TYP:	HEX(12)
		VAL:	000000000000-FFFFFFFFFFFF
	}

	FR FrameSelect OPT
	{
		CD:		'Ethernet 802.2'
		CH:		'Ethernet_802.2'
		CD:		'Ethernet 802.3'
		CH:		'Ethernet_802.3'
		CD:		'Ethernet SNAP'
		CH:		'Ethernet_SNAP'
		CD:		'Ethernet II'
		CH:		'Ethernet_II'
		DEF:	1,2
	}

}

DLANG: 4
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	6
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	7
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	8
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	14
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	12
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	9
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	10
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	1
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	16
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

LANG:	13
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."

;DrIvEr DeScRiPtIoN EnD
