;DrIvEr DeScRiPtIoN
;CoPyRiGhT=(C)Copyright Marvell. All rights reserved

VER:	1.17
SYN:	1.00

DR YUKONNW
{
	DES:		$YUKONNW_DES
	HELP:		$YUKONNW_HLP
	PAR:		2.00
	PROD:		'PCI.11AB.4320.*.*.*',
				'PCI.11AB.4360.*.*.*',
				'PCI.11AB.4361.*.*.*',
				'PCI.11AB.4362.*.*.*',
				'PCI.11AB.4350.*.*.*'

	;@#	SPROD:	'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Gigabit Ethernet 10/100/1000Base-T Controller',
	;@#			'Marvell~Yukon Fast Ethernet 10/100Base-T Controller'
	;@#	CLIENT:	YUKONNW.LAN
	;@#	ALIAS:	YUKONNW.LAN
	FILE:		YUKONNW.LAN
;	OF:			NBI.NLM, MSM.NLM, ETHERTSM.NLM
	TIME:		15

	PR SLOT REQ
	{
		VAL:	1-65535
	}

	PR NODE OPT
	{
		DES:	$NODE_DES
		HELP:	$NODE_HLP
		TYP:	HEX(12)
		VAL:	000000000000-FFFFFFFFFFFF
	}

	FR FrameSelect OPT
	{
		CD:		'Ethernet 802.2'
		CH:		'Ethernet_802.2'
		CD:		'Ethernet 802.3'
		CH:		'Ethernet_802.3'
		CD:		'Ethernet SNAP'
		CH:		'Ethernet_SNAP'
		CD:		'Ethernet II'
		CH:		'Ethernet_II'
		DEF:	1,2
	}

	PR MAXFRAMS OPT
	{
		DES:	$MAXFRAMS_DES
		HELP:	$MAXFRAMS_HLP
		TYP:	DEC(4)
		VAL:	512-9018
		DEF:	1514
		OUT:	'MAXFRAMESIZE=%s'
	}

	LI QUIET OPT
	{
		DES:	$QUIET_DES
		HELP:	$QUIET_HLP
		CD:		$QUIET_CDES1
		CH:		'ON'
		CD:		$QUIET_CDES2
		CH:		'OFF'
		CD:		$QUIET_CDES3
		CH:		'AUTO'
		DEF:	3
		OUT:	'QUIET=%s'
	}

        LI ADVTSKOFF OPT
	{
		DES:	$ADVTSKOFF_DES
		HELP:	$ADVTSKOFF_HLP
		CD:		'YES'
		CH:		''
		CD:		'NO'
		CH:		''
		DEF:	2
		OUT:	''
	}

	LI HWCSUM if (ADVTSKOFF == 2) HID
				els OPT
	{
		DES:	$HWCSUM_DES
		HELP:	$HWCSUM_HLP
		CD:		$HWCSUM_CDES1
		CH:		'ON'
		CD:		$HWCSUM_CDES2
		CH:		'OFF'
		DEF:	1
		OUT:	'HWCSUM=%s'
	}

	PR HWCSUMCAP if (ADVTSKOFF == 2) HID
				els OPT
	{
		DES:	$HWCSUMCAP_DES
		HELP:	$HWCSUMCAP_HLP
		TYP:	HEX(2)
		VAL:	0-FF
		DEF:	FF
		OUT:	'HWCSUMCAP=%s'
	}

	LI CONTYPE OPT
	{
		DES:	$CONTYPE_DES
		HELP:	$CONTYPE_HLP
		CD:		$CONTYPE_CDES1
		CH:		'AUTO'
		CD:		$CONTYPE_CDES2
		CH:		'100FD'
		CD:		$CONTYPE_CDES3
		CH:		'100HD'
		CD:		$CONTYPE_CDES4
		CH:		'10FD'
		CD:		$CONTYPE_CDES5
		CH:		'10HD'
		DEF:	1
		OUT:	'CONTYPE=%s'
	}

	LI ADVA OPT
	{
		DES:	$ADVA_DES
		HELP:	$ADVA_HLP
		CD:		'YES'
		CH:		'ON'
		CD:		'NO'
		CH:		'OFF'
		DEF:	2
		OUT:	''
	}

	LI FLWCTLA if (ADVA == 2) HID
				els OPT
	{
		DES:	$FLWCTLA_DES
		HELP:	$FLWCTLA_HLP
		CD:		$FLWCTLA_CDES1
		CH:		'NONE'
		CD:		$FLWCTLA_CDES2
		CH:		'LOCSEND'
		CD:		$FLWCTLA_CDES3
		CH:		'SYM'
		CD:		$FLWCTLA_CDES4
		CH:		'SYMORREM'
		DEF:	4
		OUT:	'FLOWCTRL_A=%s'
	}

	LI ADVP OPT
	{
		DES:	'Paced Packet Batch'
		HELP:	$ADVP_HLP
		CD:		'No Interrupt Moderation'
		CH:		'OFF'
		CD:		'Static Interrupt Moderation'
		CH:		'STATIC'
		CD:		'Dynamic Interrupt Moderation'
		CH:		'DYNAMIC'
		DEF:	1
		OUT:	''
	}

	LI MODERATE if (ADVP == 1) HID
				els REQ
	{
		DES:	$MODERATE_DES
		HELP:	$MODERATE_HLP
		CD:		$MODERATE_CDES1
		CH:		'NONE'
		CD:		$MODERATE_CDES2
		CH:		'RX'
		CD:		$MODERATE_CDES3
		CH:		'TX'
		CD:		$MODERATE_CDES4
		CH:		'BOTH'
		CD:		$MODERATE_CDES5
		CH:		'ALL'
		DEF:	1
		OUT:	'MODERATE=%s'
	}

	PR IRQPS if (ADVP == 2) REQ
				  els HID
	{
		DES:	$IRQPS_DES
		HELP:	$IRQPS_HLP
		TYP:	DEC(5)
		VAL:	1000-15000
		DEF:	5000
		OUT:	'IRQPERSEC=%s'
	}

	PR MAXIRQ if (ADVP == 3) REQ
				  els HID
	{
		DES:	$MAXIRQ_DES
		HELP:	$IRQPS_HLP
		TYP:	DEC(5)
		VAL:	1000-15000
		DEF:	5000
		OUT:	'MAXIRQPERSEC=%s'
	}

	LI ADVANCED OPT
	{
		DES:	$ADVANCED_DES
		HELP:	$ADVANCED_HLP
		CD:		'YES'
		CH:		'YES'
		CD:		'NO'
		CH:		'NO'
		DEF:	2
		OUT:	''
	}

	LI MODE if (ADVANCED == 1) OPT
				  els HID
	{
		DES:	'Mode'
		HELP:	$ADVANCED_HLP
		CD:		'Interrupt Mode'
		CH:		''
		CD:		'Polling Mode'
		CH:		'POLL'
		DEF:	1
		OUT:	'%s'
	}

	PR TXCOPYS if (ADVANCED == 1) OPT
				  els HID
	{
		DES:	$TXCOPYS_DES
		HELP:	$TXCOPYS_HLP
		TYP:	DEC(4)
		VAL:	0-9018
		DEF:	128
		OUT:	'TXCOPYSIZE=%s'
	}

	PR TXDESC1 if (ADVANCED == 1) OPT
				  els HID
	{
		DES:	$TXDES1_DES
		TYP:	DEC(3)
		VAL:	20-200
		DEF:	100
		OUT:	'TXDESC1=%s'
	}

	PR RXDESC1 if (ADVANCED == 1) OPT
				  els HID
	{
		DES:	$RXDES1_DES
		TYP:	DEC(3)
		VAL:	20-200
		DEF:	100
		OUT:	'RXDESC1=%s'
	}
}

DLANG: 4
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	6
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	7
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	8
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	14
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	12
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	9
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	10
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	1
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	16
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

LANG:	13
;Default: English
	$YUKONNW_DES =  "Marvell Yukon Ethernet Controller"
	$YUKONNW_HLP =   "This driver supports the Marvell Yukon Ethernet Controller."

	$NODE_DES =	"Node Address"
	$NODE_HLP =	"This parameter sets the locally administered
			 address. This address must be unique on the net.
			 All 12 digits must be entered!
			 Do not change this address unless you are
			 prepared to administer local addresses
			 according to IEEE 802.2 specifications. Be
			 careful not to enter a node address that is
			 already in use by another station."
	$MAXFRAMS_DES =	"Set the Maximum Frame Size"
	$MAXFRAMS_HLP =	"Setting the value above 1514 is only effective if you
			 use an ETHERTSM.NLM that supports Jumbo Frames and
			 if you load the frame type ETHERNET_II as the first
			 frame type on the specific adapter."
	$QUIET_DES =	"QUIET"
	$QUIET_HLP =	"Using this parameter status messages can be
			 supressed. This will not affect error messages."
	$QUIET_CDES1 =	"Suppress driver status messages"
	$QUIET_CDES2 =	"Don't suppress driver status messages"
	$QUIET_CDES3 =	"Auto"
	$ADVTSKOFF_DES =	"Advanced Options for Task Offload"
	$ADVTSKOFF_HLP =	"Show advanced options for task offload
                         configuration. Please read the README file before
                         changing these parameters."
	$HWCSUM_DES =	"HW Checksum"
	$HWCSUM_HLP =	"Task offload for computing checksum for Internet
                         Protocols."
	$HWCSUM_CDES1 =	"HW Checksum ON"
	$HWCSUM_CDES2 =	"HW Checksum OFF"
	$HWCSUMCAP_DES =	"HW Checksum Capabilities"
	$HWCSUMCAP_HLP =        "Task offload for computing checksum for Internet
                         Protocols."
	$ADVA_DES =	"Advanced Options"
	$ADVA_HLP =	"Show advanced options for port configuration.
			 Please read the README file before changing these
			 parameters."
	$CONTYPE_DES =  "Connection Type"
	$CONTYPE_HLP =  "This parameter sets the Speed and Duplex Mode for the
			connection"
	$CONTYPE_CDES1 =	"Auto (autonegotiation)"
	$CONTYPE_CDES2 =	"100 MBit Full Duplex (forced)"
	$CONTYPE_CDES3 =	"100 MBit Half Duplex (forced)"
	$CONTYPE_CDES4 =	" 10 MBit Full Duplex (forced)"
	$CONTYPE_CDES5 =	" 10 MBit Half Duplex (forced)"
	$FLWCTLA_DES =	"Flow Control Capability"
	$FLWCTLA_HLP =	"This parameter defines the flow control capabilities
			 the adapter will show on this port in
			 auto-negotiation process. Changing this parameter
			 may lead to a failed auto-negotiation process."
	$FLWCTLA_CDES1 =	"No Flow Control"
	$FLWCTLA_CDES2 =	"Asymmetric Flow Control to other station"
	$FLWCTLA_CDES3 =	"Symmetric Flow Control"
	$FLWCTLA_CDES4 =	"Symmetric or Asymmetric Flow Control"
	$ADVP_DES =	"Advanced Options for Paced Packet Batch"
	$ADVP_HLP =	"Show advanced options for Interrupt Moderation.
			 Please read the README file before changing these
			 parameters."
	$MODERATE_DES =	"Interrupt Moderation Mode"
	$MODERATE_HLP =	"Determines which interrupts shall be moderated"
	$MODERATE_CDES1 = "None"
	$MODERATE_CDES2 = "Moderate Receive Interrupts"
	$MODERATE_CDES3 = "Moderate Transmit Interrupts"
	$MODERATE_CDES4 = "Moderate Receive and Transmit Interrupts"
	$MODERATE_CDES5 = "Moderate all Interrupts"
	$IRQPS_DES =	"Interrupt Rate for Static Moderation."
	$IRQPS_HLP =	"Specify how many interrupts per second may occur."
	$MAXIRQ_DES =	"Interrupt Rate for Dynamic Moderation."
	$ADVANCED_DES =	"Advanced Options for Performance Tuning"
	$ADVANCED_HLP =	"Show advanced options for performance tuning
			 Please read the README file before changing these
			 parameters."
	$MODE_HLP  =	"In polling mode the adapter will not generate
			 interrupts for every received and transmitted
			 frame."
	$TXCOPYS_DES =	"Size of Transmit Copy Buffers"
	$TXCOPYS_HLP = 	"The first fragments of a frame will be copied
			 together as long as they fit into this buffer.
			 A value of 0 will disable this feature."
	$TXDES1_DES =	"Number of Transmit Descriptors"
	$RXDES1_DES =	"Number of Receive Descriptors"

;DrIvEr DeScRiPtIoN EnD
